{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["目  录","工程项目总价表(招标报表)","分类分项工程量清单计价表(招标报表+项目特征)","措施项目清单计价表(招标报表)","其他项目清单计价表(招标报表)"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"目  录","index":0,"n_rows":5,"n_cols":2,"rows_kept":5,"merged":[[0,0,0,1]],"flags":["formulas_cached_only"]}
["目  录"]
["工程项目总价表(招标报表)…………………………………………………………………………………………………","1"]
["分类分项工程量清单计价表(招标报表+项目特征)………………………………………………………………………","2"]
["措施项目清单计价表(招标报表)……………………………………………………………………………………………","55"]
["其他项目清单计价表(招标报表)……………………………………………………………………………………………","56"]

{"sheet":"工程项目总价表(招标报表)","index":1,"n_rows":13,"n_cols":6,"rows_kept":13,"merged":[[0,0,0,5],[1,0,1,3],[1,4,1,5],[2,0,2,5],[4,1,4,4],[5,1,5,4],[6,1,6,4],[7,1,7,4],[8,1,8,4],[9,1,9,4],[10,1,10,4],[11,1,11,4],[12,0,12,4],[40,0,40,5]],"flags":["formulas_cached_only"]}
["工程项目总价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
[]
["序号","工程项目名称",{"$nulls":3},"金额（元）"]
["一","分类分项工程"]
[null,"土壤改良"]
[null,"灌溉与排水"]
["二","措施项目"]
[null,"措施项目"]
["三","其他项目"]
[null,"暂列金额"]
["合     计"]

{"sheet":"分类分项工程量清单计价表(招标报表+项目特征)","index":2,"n_rows":742,"n_cols":8,"rows_kept":742,"merged":[[0,0,0,7],[1,0,1,5],[1,6,1,7],[2,0,2,7],[18,0,18,7],[19,0,19,7],[20,0,20,5],[20,6,20,7],[21,0,21,7],[32,0,32,7],[33,0,33,7],[34,0,34,5],[34,6,34,7],[35,0,35,7],[49,0,49,7],[50,0,50,7],[51,0,51,5],[51,6,51,7],[52,0,52,7],[61,0,61,7],[62,0,62,7],[63,0,63,5],[63,6,63,7],[64,0,64,7],[73,0,73,7],[74,0,74,7],[75,0,75,5],[75,6,75,7],[76,0,76,7],[89,0,89,7],[90,0,90,7],[91,0,91,5],[91,6,91,7],[92,0,92,7],[101,0,101,7],[102,0,102,7],[103,0,103,5],[103,6,103,7],[104,0,104,7],[114,0,114,7],[115,0,115,7],[116,0,116,5],[116,6,116,7],[117,0,117,7],[130,0,130,7],[131,0,131,7],[132,0,132,5],[132,6,132,7],[133,0,133,7],[143,0,143,7],[144,0,144,7],[145,0,145,5],[145,6,145,7],[146,0,146,7],[156,0,156,7],[157,0,157,7],[158,0,158,5],[158,6,158,7],[159,0,159,7],[171,0,171,7],[172,0,172,7],[173,0,173,5],[173,6,173,7],[174,0,174,7],[183,0,183,7],[184,0,184,7],[185,0,185,5],[185,6,185,7],[186,0,186,7],[199,0,199,7],[200,0,200,7],[201,0,201,5],[201,6,201,7],[202,0,202,7],[210,0,210,7],[211,0,211,7],[212,0,212,5],[212,6,212,7],[213,0,213,7],[227,0,227,7],[228,0,228,7],[229,0,229,5],[229,6,229,7],[230,0,230,7],[239,0,239,7],[240,0,240,7],[241,0,241,5],[241,6,241,7],[242,0,242,7],[257,0,257,7],[258,0,258,7],[259,0,259,5],[259,6,259,7],[260,0,260,7],[269,0,269,7],[270,0,270,7],[271,0,271,5],[271,6,271,7],[272,0,272,7],[285,0,285,7],[286,0,286,7],[287,0,287,5],[287,6,287,7],[288,0,288,7],[297,0,297,7],[298,0,298,7],[299,0,299,5],[299,6,299,7],[300,0,300,7],[312,0,312,7],[313,0,313,7],[314,0,314,5],[314,6,314,7],[315,0,315,7],[324,0,324,7],[325,0,325,7],[326,0,326,5],[326,6,326,7],[327,0,327,7],[338,0,338,7],[339,0,339,7],[340,0,340,5],[340,6,340,7],[341,0,341,7],[350,0,350,7],[351,0,351,7],[352,0,352,5],[352,6,352,7],[353,0,353,7],[366,0,366,7],[367,0,367,7],[368,0,368,5],[368,6,368,7],[369,0,369,7],[378,0,378,7],[379,0,379,7],[380,0,380,5],[380,6,380,7],[381,0,381,7],[390,0,390,7],[391,0,391,7],[392,0,392,5],[392,6,392,7],[393,0,393,7],[404,0,404,7],[405,0,405,7],[406,0,406,5],[406,6,406,7],[407,0,407,7],[420,0,420,7],[421,0,421,7],[422,0,422,5],[422,6,422,7],[423,0,423,7],[432,0,432,7],[433,0,433,7],[434,0,434,5],[434,6,434,7],[435,0,435,7],[444,0,444,7],[445,0,445,7],[446,0,446,5],[446,6,446,7],[447,0,447,7],[458,0,458,7],[459,0,459,7],[460,0,460,5],[460,6,460,7],[461,0,461,7],[472,0,472,7],[473,0,473,7],[474,0,474,5],[474,6,474,7],[475,0,475,7],[486,0,486,7],[487,0,487,7],[488,0,488,5],[488,6,488,7],[489,0,489,7],[498,0,498,7],[499,0,499,7],[500,0,500,5],[500,6,500,7],[501,0,501,7],[511,0,511,7],[512,0,512,7],[513,0,513,5],[513,6,513,7],[514,0,514,7],[525,0,525,7],[526,0,526,7],[527,0,527,5],[527,6,527,7],[528,0,528,7],[540,0,540,7],[541,0,541,7],[542,0,542,5],[542,6,542,7],[543,0,543,7],[553,0,553,7],[554,0,554,7],[555,0,555,5],[555,6,555,7],[556,0,556,7],[566,0,566,7],[567,0,567,7],[568,0,568,5],[568,6,568,7],[569,0,569,7],[579,0,579,7],[580,0,580,7],[581,0,581,5],[581,6,581,7],[582,0,582,7],[594,0,594,7],[595,0,595,7],[596,0,596,5],[596,6,596,7],[597,0,597,7],[607,0,607,7],[608,0,608,7],[609,0,609,5],[609,6,609,7],[610,0,610,7],[620,0,620,7],[621,0,621,7],[622,0,622,5],[622,6,622,7],[623,0,623,7],[634,0,634,7],[635,0,635,7],[636,0,636,5],[636,6,636,7],[637,0,637,7],[649,0,649,7],[650,0,650,7],[651,0,651,5],[651,6,651,7],[652,0,652,7],[662,0,662,7],[663,0,663,7],[664,0,664,5],[664,6,664,7],[665,0,665,7],[676,0,676,7],[677,0,677,7],[678,0,678,5],[678,6,678,7],[679,0,679,7],[690,0,690,7],[691,0,691,7],[692,0,692,5],[692,6,692,7],[693,0,693,7],[705,0,705,7],[706,0,706,7],[707,0,707,5],[707,6,707,7],[708,0,708,7],[717,0,717,7],[718,0,718,7],[719,0,719,5],[719,6,719,7],[720,0,720,7],[741,0,741,5],[741,6,741,7],[743,0,743,7]],"flags":["formulas_cached_only"]}
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
["一",null,"土壤改良\n",null," "]
[null,"500101002001","撒施有机肥 \n(100kg/亩)\n1.撒施有机肥 \n(100kg/亩)","亩","30.43"]
[null,"500101002002","撒播绿肥 (开沟播\n撒紫云英)\n1.撒播绿肥 (开沟\n播撒紫云英)","亩","311"]
["二",null,"灌溉与排水\n",null," "]
["(一)",null,"田块整治工程\n","亩","30.43"]
["1",null,"石潭镇古城村-田\n块整治工程\n","亩","30.43"]
["1.1","2025-XTXT-TZ-\nST032","TZ17-石潭镇古城\n村田块整治工程\n","亩","30.43"]
["1.1.1",null,"田块整治工程\n","项","1"]
["1.1.1.1",null,"耕作田块修筑工程\n","项","1"]
[null,"500103001001","梯田田埂修筑\n1.分层厚度及碾压\n数30cm，密实不渗\n水\n2.运距就近取土","m³","159"]
[null,"500101002003","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","4473.92"]
[null,"500103001002","土方回填（松填）\n1.土质及含水量\n:综合\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，松填","m³","4473.14"]
[null,"500103002001","保水层夯实\n1.符合设计图纸及\n规范要求","m³","4473.14"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103001003","细部平整土地\n1.符合设计图纸及\n规范要求","公顷","1.42"]
["1.1.1.2",null,"耕作层地力保持工\n程\n","项","1"]
[null,"500101002004","耕作层剥离\n1.剥离表层耕种土\n30cm以内，集中堆\n放","m³","2840.15"]
[null,"50010300001","耕作层回填\n1.表层耕植土覆盖\n30cm以内","m³","2840.15"]
["1.1.2",null,"项目区标志牌\n","项","1"]
[null,"500101002005","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","0.5"]
[null,"500109001001","C20砼垫层\n1.部位及类型:混\n凝土垫层\n2.设计龄期、强度\n等级及配合比:C20\n3.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n4.级配、拌制要求\n:满足设计强度要\n求","m³","0.13"]
[null,"500105006001","M7.5浆砌红砖\n1.品种、规格及强\n度等级:MU10页岩\n实心砖\n2.砂浆强度等级及\n配合比:M7.5水泥\n砂浆\n3.勾缝要求:满足\n设计要求","m³","1.96"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500105010001","1:2水泥砂浆抹面\n(立面)\n1.砂浆强度等级及\n配合比:1：2水泥\n砂浆\n2.抹面厚度:20mm\n3.分格缝宽度:满\n足设计要求","m²","12.49"]
[null,"500114001001","定制刻字瓷砖\n1.规格:30*45cm\n2.含制作安装等","m²","7.2"]
["(二)",null,"水源工程\n","项","1"]
["1",null,"山平塘\n","座","7"]
["1.1",null,"石潭镇古城村-山\n平塘\n","座","7"]
["1.1.1","2025-XTXT-EK-\nST1107","古城村大坝塘\n(L=120m,H=1.5m)\n砼衬砌\n","m","120"]
["1.1.1.1",null,"清淤扩容\n","项","1"]
[null,"500101002006","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³","640"]
["1.1.1.2",null,"塘堤护坡\n","m","120"]
[null,"500101002007","外坡除杂\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","180"]
[null,"500101002008","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","111.6"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103001004","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","20.4"]
[null,"500109001002","C25砼截水墙\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","28.8"]
[null,"500109001003","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","36"]
[null,"500109009001","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","6.9"]
[null,"500110001001","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","504"]
[null,"500114001002","标识牌\n1.满足设计要求","处","1"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103010001","基础处理\n1.颗粒级配:人工\n抛石护底护岸 胶\n轮车运\n2.厚度:200mm","m³","67.2"]
["1.1.1.3",null,"溢洪道\n","m","6"]
[null,"500101002009","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","2.94"]
[null,"500103001005","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","2.1"]
[null,"500109001004","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.6"]
[null,"500109001005","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.72"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001002","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","15.6"]
["1.1.1.4","500114002001","抽水台班\n1.潜水泵 功率\n2.2kW","台班","4"]
["1.1.1.5","500114001003","水位尺\n1.满足设计要求","根","3"]
["1.1.2","2025-XTXT-EK-\nST1108","古城村萧家上塘\n(L=300m,H=2.5m)\n砼衬砌\n","m","300"]
["1.1.2.1",null,"清淤扩容\n","项","1"]
[null,"500101002010","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³"," "]
[null,"500101002006","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³","2000"]
["1.1.2.2",null,"塘堤护坡\n","m","300"]
[null,"500101002011","外坡除杂\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","750"]
[null,"500101002012","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","345"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103001006","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","174"]
[null,"500109001006","C25砼截水墙\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","36"]
[null,"500109001007","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","81"]
[null,"500103007001","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","81"]
[null,"500109009002","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","15.93"]
[null,"500109011001","C25砼踏步\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.86"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001003","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","240"]
[null,"500114001004","标识牌\n1.满足设计要求","处","1"]
[null,"500103010002","基础处理\n1.颗粒级配:人工\n抛石护底护岸 胶\n轮车运\n2.厚度:200mm","m³","168"]
["1.1.2.3",null,"溢洪道\n","m","6"]
[null,"500101002013","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","2.94"]
[null,"500103001007","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","2.1"]
[null,"500109001008","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.6"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001009","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.72"]
[null,"500110001004","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","15.6"]
["1.1.2.4","500114002002","抽水台班\n1.潜水泵 功率\n2.2kW","台班","4"]
["1.1.2.5","500114001005","水位尺\n1.满足设计要求","根","3"]
["1.1.3","2025-XTXT-EK-\nST1109","古城村萧家下塘\n(L=300m,H=2.5m)\n砼衬砌\n","m","300"]
["1.1.3.1",null,"清淤扩容\n","项","1"]
[null,null,"\n",null," "]
[null,"500101002014","清淤（外运1km、\n就地处理）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³"," "]
[null,"500101002006","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³","2000"]
["1.1.3.2",null,"塘堤护坡\n","m","300"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500101002015","外坡除杂\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","750"]
[null,"500101002016","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","345"]
[null,"500103001008","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","174"]
[null,"500109001010","C25砼截水墙\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","36"]
[null,"500109001011","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","81"]
[null,"500103007002","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","81"]
[null,"500109009003","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","15.93"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109011002","C25砼踏步\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.86"]
[null,"500110001005","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","240"]
[null,"500114001006","标识牌\n1.满足设计要求","处","1"]
[null,"500103010003","基础处理\n1.颗粒级配:人工\n抛石护底护岸 胶\n轮车运\n2.厚度:200mm","m³","168"]
["1.1.3.3",null,"溢洪道\n","m","6"]
[null,"500101002017","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","2.94"]
[null,"500103001009","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","2.1"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001012","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.6"]
[null,"500109001013","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.72"]
[null,"500110001006","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","15.6"]
["1.1.3.4","500114002003","抽水台班\n1.潜水泵 功率\n2.2kW","台班","4"]
["1.1.3.5","500114001007","水位尺\n1.满足设计要求","根","3"]
["1.1.4","2025-XTXT-EK-\nST1110","古城村大瓦塘\n(L=210m,H=1.5m)\n砼衬砌\n","m","210"]
["1.1.4.1",null,"清淤扩容\n","项","1"]
[null,"500101002018","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³","1040"]
["1.1.4.2",null,"塘堤护坡\n","m","210"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500101002019","外坡除杂\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","315"]
[null,"500101002020","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","195.3"]
[null,"500103001010","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","35.7"]
[null,"500109001014","C25砼截水墙\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","50.4"]
[null,"500109001015","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","63"]
[null,"500109009004","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","12.3"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001007","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","882"]
[null,"500114001008","标识牌\n1.满足设计要求","处","1"]
[null,"500103010004","基础处理\n1.颗粒级配:人工\n抛石护底护岸 胶\n轮车运\n2.厚度:200mm","m³","117.6"]
["1.1.4.3","500114002004","抽水台班\n1.潜水泵 功率\n2.2kW","台班","4"]
["1.1.4.4","500114001009","水位尺\n1.满足设计要求","根","3"]
["1.1.5","2025-XTXT-EK-\nST1111","古城村石马上塘\n(L=70m,H=1.8m)\n砼衬砌\n","m","70"]
["1.1.5.1",null,"清淤扩容\n","项","1"]
[null,"500101002021","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³","480"]
["1.1.5.2",null,"内坡M7.5浆砌石护\n坡 \n","m","70"]
[null,"500101002022","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","309.12"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103001011","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","162.96"]
[null,"500105003001","M7.5浆砌石侧墙\n1.品种、规格及强\n度等级:MU30块石\n2.砂浆强度等级及\n配合比:M7.5水泥\n砂浆\n3.勾缝要求:满足\n设计要求","m³","97.02"]
[null,"500105003002","M7.5浆砌石基础\n1.品种、规格及强\n度等级:MU30块石\n2.砂浆强度等级及\n配合比:M7.5水泥\n砂浆\n3.满足设计要求","m³","43.4"]
[null,"500109001016","C25砼压顶\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","3.5"]
[null,"500103005001","反滤体\n1.颗粒级配:天然\n级配","m³","0.35"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001008","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","m²","14"]
[null,"500109009005","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","12.69"]
[null,"500112004001","Φ50PVC排水管\n1.Φ50PVC排水管\n制安","处","33.25"]
[null,"500114001010","标识牌\n1.满足设计要求","处","1"]
[null,"500103010005","基础处理\n1.颗粒级配:人工\n抛石护底护岸 胶\n轮车运\n2.厚度:200mm","m³","28"]
["1.1.5.3","500114002005","抽水台班\n1.潜水泵 功率\n2.2kW","台班","4"]
["1.1.5.4","500114001011","水位尺\n1.满足设计要求","根","3"]
["1.1.6","2025-XTXT-EK-\nST1112","古城村石马下塘\n(L=40m,H=1.8m)\n砼衬砌\n","m","40"]
["1.1.6.1",null,"清淤扩容\n","项","1"]
[null,"500101002023","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³","480"]
["1.1.6.2",null,"内坡M7.5浆砌石护\n坡 \n","m","40"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500101002024","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","176.64"]
[null,"500103001012","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","93.12"]
[null,"500105003003","M7.5浆砌石侧墙\n1.品种、规格及强\n度等级:MU30块石\n2.砂浆强度等级及\n配合比:M7.5水泥\n砂浆\n3.勾缝要求:满足\n设计要求","m³","55.44"]
[null,"500105003004","M7.5浆砌石基础\n1.品种、规格及强\n度等级:MU30块石\n2.砂浆强度等级及\n配合比:M7.5水泥\n砂浆\n3.满足设计要求","m³","24.8"]
[null,"500109001017","C25砼压顶\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","2"]
[null,"500103005002","反滤体\n1.颗粒级配:天然\n级配","m³","0.2"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001009","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","m²","8"]
[null,"500109009006","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","6.37"]
[null,"500112004002","Φ50PVC排水管\n1.Φ50PVC排水管\n制安","处","19"]
[null,"500114001012","标识牌\n1.满足设计要求","处","1"]
[null,"500103010006","基础处理\n1.颗粒级配:人工\n抛石护底护岸 胶\n轮车运\n2.厚度:200mm","m³","16"]
["1.1.6.3","500114002006","抽水台班\n1.潜水泵 功率\n2.2kW","台班","4"]
["1.1.6.4","500114001013","水位尺\n1.满足设计要求","根","3"]
["1.1.7","2025-XTXT-EK-\nST1113","古城村菜篮子塘\n(L=310m,H=1.2m)\n砼衬砌\n","m","310"]
["1.1.7.1",null,"清淤扩容\n","项","1"]
[null,"500101002025","清淤（外运1km）\n1.挖机挖淤泥\n2.运距暂按1km考\n虑","m³","1500"]
["1.1.7.2",null,"塘堤护坡\n","m","310"]
[null,"500101002026","外坡除杂\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","372"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500101002027","土方开挖\n1.土类土方类别综\n合\n2.开挖厚度依据土\n方平衡\n3.运距场内运输","m³","260.4"]
[null,"500103001013","土方回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","43.4"]
[null,"500109001018","C25砼截水墙\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","74.4"]
[null,"500109001019","C25砼护坡\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","86.8"]
[null,"500103007001","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","43.4"]
[null,"500109009007","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","14.64"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001010","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","1116"]
[null,"500114001014","标识牌\n1.满足设计要求","处","1"]
[null,"500103010007","基础处理\n1.颗粒级配:人工\n抛石护底护岸 胶\n轮车运\n2.厚度:200mm","m³","173.6"]
["1.1.7.3","500114002007","抽水台班\n1.潜水泵 功率\n2.2kW","台班","4"]
["1.1.7.4","500114001015","水位尺\n1.满足设计要求","根","3"]
["(三)",null,"输水工程\n","m","2230"]
["1",null,"石潭镇古城村-输\n水工程\n","m","2230"]
["1.1","2025-XTXT-QG-\nST409","QG-\nST409(0.6m*0.6m\n)\n","m","430"]
["1.1.1",null,"渠道部分\n","m","430"]
[null,"500101002028","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","219.3"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103001014","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","86.86"]
[null,"500103007003","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","32.25"]
[null,"500109001020","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","32.25"]
[null,"500109001021","C25砼渠道护坡（\n10cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","54.18"]
[null,"500110001011","钢模板制安\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","541.8"]
[null,"500109009008","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","17.09"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500112004003","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","43"]
[null,"500101002029","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","860"]
[null,"500103014001","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","322.5"]
[null,"500114001016","水位尺\n1.满足设计要求","根","1"]
[null,"500114001017","标识牌\n1.满足设计要求","处"," "]
["1.1.2",null,"分水口（0.6m）\n","处","8"]
[null,"500101002030","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","6.46"]
[null,"500103001015","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","5.04"]
[null,"500109001022","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.16"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001012","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","8.15"]
[null,"500202005001","木闸门\n1.满足设计要求","m²","9"]
["1.1.3",null,"人行桥（0.6m）\n","座","4"]
[null,"500109001023","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.84"]
[null,"500109001024","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","2.61"]
[null,"500110001013","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","18.16"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500111002001","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.16"]
["1.1.4",null,"机耕桥（0.6m）\n","座","4"]
[null,"500109001025","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.12"]
[null,"500109001026","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","5.22"]
[null,"500110001014","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","22.96"]
[null,"500111002002","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.16"]
["1.2","2025-XTXT-QG-\nST410","QG-\nST410(0.5m*0.5m\n)\n","m","340"]
["1.2.1",null,"渠道部分\n","m","340"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500101002031","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","214.2"]
[null,"500103001016","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","119"]
[null,"500103007004","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","23.8"]
[null,"500109010001","砼拆除\n1.机械拆除混凝土\n2.自卸汽车运1km","m³","32.64"]
[null,"500109001027","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","23.8"]
[null,"500109001028","C25砼渠道护坡（\n10cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","34"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001015","钢模板制安\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","612"]
[null,"500109009009","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","12.73"]
[null,"500112004004","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","34"]
[null,"500101002032","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","680"]
[null,"500103014002","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","238"]
[null,"500114001018","水位尺\n1.满足设计要求","根","1"]
[null,"500114001019","标识牌\n1.满足设计要求","处"," "]
["1.2.2",null,"分水口（0.5m）\n","处","6"]
[null,"500101002033","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","3.26"]
[null,"500103001017","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","1.95"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001029","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.75"]
[null,"500110001016","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","5.14"]
[null,"500202005002","木闸门\n1.满足设计要求","m²","4.85"]
["1.2.3",null,"人行桥（0.5m）\n","座","3"]
[null,"500109001030","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.56"]
[null,"500109001031","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.63"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001017","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","11.74"]
[null,"500111002003","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.09"]
["1.2.4",null,"机耕桥（0.5m）\n","座","3"]
[null,"500109001032","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.49"]
[null,"500109001033","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","3.26"]
[null,"500110001018","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","14.81"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500111002004","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.09"]
["1.3","2025-XTXT-QG-\nST411","QG-\nST411(0.6m*0.6m\n)\n","m","370"]
["1.3.1",null,"渠道部分\n","m","370"]
[null,"500101002034","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","188.7"]
[null,"500103001018","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","74.74"]
[null,"500103007005","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","27.75"]
[null,"500109001034","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","27.75"]
[null,"500109010002","砼拆除\n1.机械拆除混凝土\n2.自卸汽车运1km","m³","53.28"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001035","C25砼渠道护坡（\n10cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","46.62"]
[null,"500110001019","钢模板制安\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","466.2"]
[null,"500109009010","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","14.67"]
[null,"500112004005","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","37"]
[null,"500101002035","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","740"]
[null,"500103014003","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","277.5"]
[null,"500114001020","水位尺\n1.满足设计要求","根","1"]
[null,"500114001021","标识牌\n1.满足设计要求","处","1"]
["1.3.2",null,"分水口（0.6m）\n","处","7"]
[null,"500101002036","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","5.66"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103001019","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","4.41"]
[null,"500109001036","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.02"]
[null,"500110001020","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","7.13"]
[null,"500202005003","木闸门\n1.满足设计要求","m²","7.87"]
["1.3.3",null,"人行桥（0.6m）\n","座","3"]
[null,"500109001037","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.63"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001038","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.96"]
[null,"500110001021","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","13.62"]
[null,"500111002005","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.12"]
["1.3.4",null,"机耕桥（0.6m）\n","座","3"]
[null,"500109001039","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.84"]
[null,"500109001040","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","3.91"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500110001022","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","17.22"]
[null,"500111002006","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.12"]
["1.4","2025-XTXT-QG-\nST412","QG-\nST412(0.5m*0.5m\n)\n","m","300"]
["1.4.1",null,"渠道部分\n","m","300"]
[null,"500101002037","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","189"]
[null,"500103001020","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","105"]
[null,"500103007006","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","21"]
[null,"500109010003","砼拆除\n1.机械拆除混凝土\n2.自卸汽车运1km","m³","36"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001041","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","21"]
[null,"500109001042","C25砼渠道护坡（\n10cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","30"]
[null,"500110001023","钢模板制安\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","540"]
[null,"500109009011","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","11.21"]
[null,"500112004006","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","30"]
[null,"500101002038","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","600"]
[null,"500103014004","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","210"]
[null,"500114001022","水位尺\n1.满足设计要求","根","1"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500114001023","标识牌\n1.满足设计要求","处","1"]
["1.4.2",null,"分水口（0.5m）\n","处","6"]
[null,"500101002039","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","3.26"]
[null,"500103001021","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","1.95"]
[null,"500109001043","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.75"]
[null,"500110001024","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","5.14"]
[null,"500202005004","木闸门\n1.满足设计要求","m²","4.85"]
["1.4.3",null,"人行桥（0.5m）\n","座","3"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001044","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.56"]
[null,"500109001045","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.63"]
[null,"500110001025","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","11.74"]
[null,"500111002007","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.09"]
["1.4.4",null,"机耕桥（0.5m）\n","座","3"]
[null,"500109001046","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.49"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001047","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","3.26"]
[null,"500110001026","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","14.81"]
[null,"500111002008","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.09"]
["1.5","2025-XTXT-QG-\nST413","QG-\nST413(0.4m*0.4m\n)\n","m","270"]
["1.5.1",null,"渠道部分\n","m","270"]
[null,"500101002040","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","135"]
[null,"500103001022","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","81"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103007007","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","16.2"]
[null,"500109001048","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","16.2"]
[null,"500109010004","砼拆除\n1.机械拆除混凝土\n2.自卸汽车运1km","m³","25.92"]
[null,"500109001049","C25砼渠道护坡（\n10cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","21.6"]
[null,"500110001027","钢模板制安\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","486"]
[null,"500109009012","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","7.42"]
[null,"500112004007","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","27"]
[null,"500101002041","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","540"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103014005","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","162"]
[null,"500114001024","标识牌\n1.满足设计要求","处","1"]
[null,"500114001025","水位尺\n1.满足设计要求","根","1"]
["1.5.2",null,"分水口（0.4m）\n","处","5"]
[null,"500101002042","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","1.9"]
[null,"500103001023","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","0.9"]
[null,"500109001050","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.39"]
[null,"500110001028","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","4.03"]
[null,"500202005005","木闸门\n1.满足设计要求","m²","1.62"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
["1.5.3",null,"人行桥（0.4m）\n","座","2"]
[null,"500109001051","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.24"]
[null,"500109001052","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.52"]
[null,"500110001029","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","6.68"]
[null,"500111002009","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.04"]
["1.5.4",null,"机耕桥（0.4m）\n","座","2"]
[null,"500109001053","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.48"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001054","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.04"]
[null,"500110001030","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","12.08"]
[null,"500111002010","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.04"]
["1.6","2025-XTXT-QG-\nST414","QG-\nST414(0.4m*0.4m\n)\n","m","160"]
["1.6.1",null,"渠道部分\n","m","160"]
[null,"500101002043","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","80"]
[null,"500103001024","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","48"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103007008","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","9.6"]
[null,"500109001055","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","9.6"]
[null,"500109001056","C25砼渠道护坡（\n10cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","12.8"]
[null,"500110001031","钢模板制安\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","288"]
[null,"500109009013","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","4.34"]
[null,"500112004008","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","16"]
[null,"500101002044","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","320"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103014006","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","96"]
[null,"500114001026","标识牌\n1.满足设计要求","处","1"]
[null,"500114001027","水位尺\n1.满足设计要求","根","1"]
["1.6.2",null,"分水口（0.4m）\n","处","3"]
[null,"500101002045","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","1.14"]
[null,"500103001025","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","0.54"]
[null,"500109001057","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.23"]
[null,"500110001032","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","2.42"]
[null,"500202005006","木闸门\n1.满足设计要求","m²","0.97"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
["1.6.3",null,"人行桥（0.4m）\n","座","1"]
[null,"500109001058","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.12"]
[null,"500109001059","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.26"]
[null,"500110001033","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","3.34"]
[null,"500111002011","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.02"]
["1.6.4",null,"机耕桥（0.4m）\n","座","1"]
[null,"500109001060","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.24"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001061","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.52"]
[null,"500110001034","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","6.04"]
[null,"500111002012","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.02"]
["1.7","2025-XTXT-QG-\nST415","QG-\nST415(0.4m*0.4m\n)\n","m","110"]
["1.7.1",null,"渠道部分\n","m","110"]
[null,"500101002046","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","55"]
[null,"500103001026","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","33"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103007009","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","6.6"]
[null,"500109001062","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","6.6"]
[null,"500109010005","砼拆除\n1.机械拆除混凝土\n2.自卸汽车运1km","m³","10.56"]
[null,"500109001063","C25砼渠道护坡（\n10cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","8.8"]
[null,"500110001035","钢模板制安\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","198"]
[null,"500109009014","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","2.94"]
[null,"500112004009","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","11"]
[null,"500101002047","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","220"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500103014007","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","66"]
[null,"500114001028","标识牌\n1.满足设计要求","处","1"]
[null,"500114001029","水位尺\n1.满足设计要求","根","1"]
["1.7.2",null,"分水口（0.4m）\n","处","2"]
[null,"500101002048","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","0.76"]
[null,"500103001027","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","0.36"]
[null,"500109001064","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.16"]
[null,"500110001036","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","1.61"]
[null,"500202005007","木闸门\n1.满足设计要求","m²","0.65"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
["1.7.3",null,"人行桥（0.4m）\n","座","1"]
[null,"500109001065","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.12"]
[null,"500109001066","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.26"]
[null,"500110001037","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","3.34"]
[null,"500111002013","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.02"]
["1.7.4",null,"机耕桥（0.4m）\n","座","1"]
[null,"500109001067","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.24"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001068","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.52"]
[null,"500110001038","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","6.04"]
[null,"500111002014","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.02"]
["1.8","2025-XTXT-QG-\nST416","QG-ST416(2m*1m)\n","m","250"]
["1.8.1",null,"渠道部分\n","m","250"]
[null,"500101002049","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","367.5"]
[null,"500103001028","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","122.5"]
[null,"500103007010","砂石垫层\n1.颗粒级配:天然\n级配砂卵石\n2.厚度:100mm","m³","57.5"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001069","C25砼底板(10cm)\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","57.5"]
[null,"500109001070","C25砼渠道护坡（\n15cm）\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","78"]
[null,"500109010006","砼拆除\n1.机械拆除混凝土\n2.自卸汽车运1km","m³","80"]
[null,"500110001039","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","520"]
[null,"500109009015","沥青杉木板伸缩缝\n1.伸缩缝 沥青杉\n板(厚度2cm)","m²","21.17"]
[null,"500112004010","DN200PVC排水管\n1.DN200PVC排水管\n安装","m","250"]
[null,"500101002050","清表\n1.清除表层杂草、\n虚土等杂质\n2.就近堆放","m²","500"]
[null,"500103014008","渠底彩条布\n1.材质:彩条布\n2.铺设牢固无破损\n，松弛度合适","m²","575"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500114001030","水位尺\n1.满足设计要求","根","1"]
[null,"500114001031","标识牌\n1.满足设计要求","处","1"]
["1.8.2",null,"分水口（2.0m）\n","处","5"]
[null,"500101002051","渠道土方开挖\n1.土方类别综合\n2.就近堆放","m³","13.38"]
[null,"500103001029","土方沟槽回填夯实\n1.土质及含水量\n:就近取土\n2.分层厚度及碾压\n数:分层填筑，每\n层厚度不大于\n30cm，压实度不应\n小于0.94\n3.填筑体干密度、\n透系数:符合设计\n图纸及规范要求","m³","6.82"]
[null,"500109001071","C25砼闸墩\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","1.53"]
[null,"500110001040","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","7.76"]
[null,"500202005008","木闸门\n1.满足设计要求","m²","12.52"]
["1.8.3",null,"人行桥（2.0m）\n","座","2"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001072","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","0.93"]
[null,"500109001073","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","5.68"]
[null,"500110001041","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","17.62"]
[null,"500111002015","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.08"]
["1.8.4",null,"机耕桥（2.0m）\n","座","2"]
[null,"500109001074","C35砼桥板\n1.设计龄期、强度\n等级及配合比:C35\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","2.48"]
[]
[]
["分类分项工程量清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
["序号","项目编码","项目名称","计量\n单位"," 工程\n 数量","单价\n(元)","合价\n(元)","主要技术\n条款编码"]
[null,"500109001075","C25桥台砼\n1.设计龄期、强度\n等级及配合比:C25\n2.抗渗、抗冻、抗\n磨等要求:符合设\n计图纸及规范要求\n3.级配、拌制要求\n:满足设计强度要\n求","m³","5.68"]
[null,"500110001042","钢模板\n1.类型及结构尺寸\n:承包商结合现有\n施工工艺自行考虑\n2.制作、组装、安\n装及拆卸标准(如\n强度、刚度、稳定\n性):普通模板，含\n模板制作、安装、\n拆除、归堆整理等\n工作内容","㎡","34.4"]
[null,"500111002016","钢筋制安\n1.钢筋制作与安装\n2.型号、规格:综\n合","t","0.14"]
{"$rows_empty":16}
["合      计"]

{"sheet":"措施项目清单计价表(招标报表)","index":3,"n_rows":39,"n_cols":6,"rows_kept":39,"merged":[[0,0,0,5],[1,0,1,3],[1,4,1,5],[2,0,2,5],[4,1,4,3],[5,1,5,3],[6,1,6,3],[7,1,7,3],[8,1,8,3],[9,1,9,3],[10,1,10,3],[11,1,11,3],[12,1,12,3],[13,1,13,3],[14,1,14,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[18,1,18,3],[19,1,19,3],[20,1,20,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[27,1,27,3],[28,1,28,3],[29,1,29,3],[30,1,30,3],[31,1,31,3],[32,1,32,3],[33,1,33,3],[34,1,34,3],[35,1,35,3],[36,1,36,3],[37,1,37,3],[38,1,38,4],[40,0,40,5]],"flags":["formulas_cached_only"]}
["措施项目清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
[]
["序号","项 目 名 称",null,null,"单位","金额"]
[null,"措施项目",{"$nulls":3},"47415.5"]
[null,"安全文明施工措施费",null,null,"项","42415.5"]
[null,"施工场地费",null,null,"项","5000"]
{"$rows_empty":30}
[null,"合                计",{"$nulls":3},"47415.5"]

{"sheet":"其他项目清单计价表(招标报表)","index":4,"n_rows":39,"n_cols":5,"rows_kept":39,"merged":[[0,0,0,4],[1,0,1,2],[1,3,1,4],[2,0,2,4],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[40,0,40,4]],"flags":["formulas_cached_only"]}
["其他项目清单计价表"]
["合同编号："]
["工程名称：湘潭县2025年高标准农田建设项目（投融资创新）第44标 "]
[]
["序号","项目名称",null,"金额(元)","备注"]
[null,"暂列金额",null,"85975.38"]
[null,"不可预计费",null,"85975.38"]
{"$rows_empty":31}
[null,"合     计",null,"85975.38"]